Version number:     Ver1.16
Product Line:       Moxa Smartio/Industio/UPCI/PCIe/"PC/104-Plus" Family
Platform:           x86, x64, Linux kernel 2.4.x, 2.6.x, 3.x & above
Company:            Moxa Inc.
Date:               03/03/2014

Supported Product:
====================
CP-102U, CP-102UL, CP-102UF
CP-132U-I, CP-132UL,
CP-132, CP-132I, CP132S, CP-132IS, 
CI-132, CI-132I, CI-132IS, 
(C102H, C102HI, C102HIS, C102P, CP-102, CP-102S)

CP-104EL, CP-104UL, CP-104JU,
CP-134U, CP-134U-I
C104H/PCI, C104HS/PCI, 
CP-114, CP-114I, CP-114S, CP-114IS, CP-114UL
C104H, C104HS, 
CI-104J, CI-104JS
CI-134, CI-134I, CI-134IS, 
(C114HI, CT-114I, C104P)

CP-118EL, CP-118U, CP-118U-I,
CP-138U, CP-138U-I
CP-168EL, CP-168U,
C168H/PCI,  
C168H, C168HS, 
(C168P)

CB-108, CB-114, CB-134I

POS-104UL

CP-102E, CP-102EL, CP-132EL, CP-132EL-I, CP-114EL, CP-114EL-I

CP-112UL, CP-112UL-I, CP-114UL-I

CP-104EL-A, CP-168EL-A, CP-118EL-A, CP-118E-I-A

CP-134EL-A-I, CP-118E-A-I, CP-138E-A-I, CP-116E-A

Release Note:
=============
ver1.16 Build 14030317 (03/03/2014)
1. New: Support new models CP-134EL-A-I, CP-118E-A-I, CP-138E-A-I, CP-116E-A.
2. New: Enable Smart RS-485 function of new supported models.
3. New: Support kernel version up to 3.11.0
4. New: Support distribution Fedora 16 (Kernel 3.1.1)
5. New: Support linear baud for MUE250/MUE450/MUE850.
6. Improve: The PCI-E modules now support disable FIFO feature	 
7. Bugfix: Compile error in Debian7
8. Bugfix: The data transmission not stop after port close with low baudrate.
9. Bugfix: The serial settings not set when serial port open.
10. Bugfix: Fix the size problem of ioctl 'TIOCSERGETLSR' in 64-bit kernel 
11. Bugfix: Fix the prototype of IOCTL operation declare improperly on
    linux kernel 3.x
12. Bugfix: Fix system crash when application calls ioctl() with TIOCMIWAIT.

Ver1.15
1. Add CP-104EL-A, CP-168EL-A, CP-118EL-A, CP-118E-I-A.
2. Support kernel up to 2.6.30.
3. Fix msdiag utility in x64 system.

Ver1.14
1. Support kernel up to 2.4.37.
2. Add CP-112UL, CP-112UL-I, CP-114UL-I.
3. Fix a problem of msmknod which can't execute in CSH.
4. Support kernel up to 2.6.28.
5. Support kernel up to 2.6.27.
6. Support kernel up to 2.6.26.
7. Modify some content of build.log and add Moxa email support@moxa.com. 

Ver1.13
1. Add CP-102E, CP-102EL, CP-132E, CP-132EL-I, CP-114EL, CP-114EL-I.

Ver1.12
1. Add CP-102UF model.
2. Support kernel up to 2.6.21.
3. Support to set baud rate by setserial.

Ver1.11
1. Add CP-114UL model. 

Ver1.10
1. Add seven models.
   CB-108, CB-114, CB-134I, CP-118U-I, CP-138U, CP-138U-I, POS-104UL
2. Support kernel up to 2.6.20.
3. Support Fedora Core 6.
4. Fix the problem that the driver can't install into the kernel.
5. Fix the "backspace" and "delete" keys of msterm.
6. Fix the problem that the system hangs up while opening the moxa
   card with minicom.
7. Fix the error that the echo function failed to send string.
8. Support kernel up to 2.6.18, including Fedora Core 5.
9. Fix the error installation of port numbers.
	In previous version of driver, if the card is not 8 ports product, the driver will assign it as 4 ports product.
	Therefore, the driver recognized incorrect port numbers in all 2 ports ISA products.
	The bug is at the mxser_get_ISA_conf() function.
10. Support non-standard baud rate.
11. Programming guide for special baud rate:
	
   - Define the I/O control code.
    
	 #define  MOXA_SET_SPECIAL_BAUD_RATE  0x44D 	
	
   - Using the ioctl() API to set non-standard baud rate after 
     setting the termios parameters.
	  
	 int  baud; 
	 baud = 500000;  /* set the non-standard baud rate */
	 ...
	 tcsetattr(fd,TCSANOW,&t);

	 ioctl(fd, MOXA_SET_SPECIAL_BAUD_RATE, &baud); 
12. Support kernel up to 2.6.17rc1, including Fedora Core 5.

Ver1.9
1. Support x64 Linux edition.
2. Support CP-118EL, CP-168EL, CP-104EL PCI Express board
3. Fix data lost problem which caused by race condition.
4. Use access_ok() to replace verify_area() begin kernel 2.6.
5. Fixed depmod failed problem under RHEL AS 3.
6. Remove 1.8.10 debug messages.
7. Add debug info (You can see it in /var/log/messages).   
8. TCSADRAIN TCSAFLUSH will flush the output queued data. Fixed.
9. Modify mxser_write to Support 2.6.10 or above.
10. Under 2.6.10, the ttyMx need to be created at each boot. You 
   can see rc.mxser for reference.
11. Redefine some function prototype without defining "inline".
   - mxser_receive_chars()
   - mxser_transmit_chars()
   - mxser_check_modem_status()
12. Fix system halt problem under SuSE 9.1 +2.6.5-7.108smp.

Ver1.8
1. Offical Release.
2. In this version, use "modprobe mxser" to load driver instead.
3. Speed up msmon load time.
4. Fix system halt problem while traffic is heavy (for ver1.7.7).
5. Fix low performance problem on PCI board (for ver1.7.7). 
6. Linux 2.0.x & 2.2.x doesn't support any more from this version.
7. cum* device is obsolete under Linux kernel 2.6 (but still also
   availabe under Linux kernel 2.4). Use ttyM* device instead.
8. Support MOXA powered UART MU860. This can enhance CP-168U/CP-104U/
   CP-104JU v2 performance & function (on-chip SW flow control,
   up to 921.6k baud rate, 128 bytes FIFO).
9. Newly support CP-118U, CP-102U, CP-102UL.  
10. Support Linux 2.6.x.
    a. For RedHat AS/ES/WS/Fedora Core 1 (not for Core 2):
	 # make installsp1 
    b. Use "insmod ./mxser.ko" under mxser\driver, not "insmod mxser".
11. Fixed the Tx/Rx problem when using ISA Boards.
12. Fix compiling problem under Red Hat AS/ES/WS/Fedora Core 1.
    To fix this problem, the compiling option must be changed from "install" 
    to "installsp1". 

   - original -
	# cd <installed> directory
	# make install 
	# ...

   - new -
	# cd <installed> directory
	# make installsp1 
	# ...


-End-
