
Product:	Moxa Smartio/Industio Windows Driver
Version:	1.24
Date:		08/30/2017
Company:	Moxa Inc.

Support Platform:
-----------------
Windows 2000
Windows XP    (x86/x64)
Windows Vista (x86/x64)
Windows Server 2003 (x86/x64)
Windows Server 2008 (x86/x64)

Supported Moxa Product:
------------------------
CA-104, CA-132, CA-132I, CA-108, CA-114, CA-134I
CB-108, CB-114, CB-134I

CP-102E, CP-102EL, CP-132EL, CP-132EL-I
CP-102U, CP-102UL
CP-132UL-I, CP-132UL,
CP-132, CP-132I, CP132S, CP-132IS, 
CI-132, CI-132I, CI-132IS, 
CP-102UF-S, CP-102UF-M
(C102H, C102HI, C102HIS, C102P, CP-102, CP-102S)

CP-114EL, CP-114EL-I
CP-104EL, CP-104UL, CP-104JU, CP-104EL-A
CP-134U, CP-134U-I, CP-134EL-A-I
C104H/PCI, C104HS/PCI, 
CP-114, CP-114I, CP-114S, CP-114IS,
C104H, C104HS, 
CI-104J, CI-104JS
CI-134, CI-134I, CI-134IS, 
(C114HI, CT-114I, C104P)

CP-118EL, CP-118U, CP-118EL-A, CP-118E-A-I
CP-138E-A-I
CP-168EL, CP-168U, CP-168EL-A
C168H/PCI,  
C168H, C168HS, 
(C168P)

CP-118U-I, CP-138U, CP-138U-I
POS-104UL

CP-114UL, CP-114UL-I
CP-112UL, CP-112UL-I

CP-116E-A

Release Note:
--------------
Ver1.24 Build 17083014
1. New: Support PC/104 serial boards.
2. Change: Windows XP is not supported in WHQL Testing anymore.
3. Bugfix: Fixed that data out of sequence under Windows 10 for PCIe card.
4. Bugfix: Fixed that RTS toggle is not working for PCIe boards.
5. Bugfix: Fixed Model name cannot be listed in the Add New Hardware Wizard 
6. Bugfix: Fixed ISA card cannot be installed.
7. Bugfix: Fixed BSOD which occurs when driver cancels the pending IRPs.
8. Bugfix: Solve communication problem randomly happened after system boots up
           with CP134EL-A-I, CP138E-A-I, CP118E-A-I, and CP-116E-A.
           
Ver1.23 Build 16010511
1. New: Support Windows 10
2. New: Driver installation can be finished by Windows driver setup wizard.
3. Improve: The number of cards each PC can support now is increased to 8.
4. Bugfix: Fix the issue that user can not open two property pages of driver
           configuration simutaneously.
5. Bugfix: Fixed CP-116E-A cannot be installed when the maximum number of
           board in a system is not achieve.
6. Bugfix: Fix Termination Resistor cannot be changed when interface is RS-422
           and RS-485 4W.		  
7. Bugfix: Fix PCIe boards might fail to run in BurnInTest utility.
8. Bugfix: The TX/RX FIFO of PCIe MSB may not be flushed when port is closed.
9. Bugfix: BSOD on some platforms.

Ver1.22 Build 14030711
1. New: Support CP134EL-A-I, CP118E-A-I, CP138E-A-I and CP-116E-A

Ver1.21 Build 14010913
1. New: Support Windows 8.1
2. New: Support Windows Server 2012 R2
3. Bugfix: The serial mouse may not work as system restore from sleep. 
4. Bugfix: Fixed driver cannot be installed due to signature issue.

Ver1.20 Build 12111310
1. New: Support Windows 8
2. New: Support Windows Server 2012
3. Improve: Allow to use IOCTL_SERIAL_SET_FIFO_CONTROL to clear RX FIFO
           (with value 0x02) or TX FIFO (with value 0x04.)
4. Bugfix: Flush TX FIFO more times to prevent serial port send unknown data 
           out when application close port
5. Bugfix: Fixed the bug that linear baudrate not support below 200 bps

Ver1.19 Build 11062215
1.  New: Support linear baud rate for MUE-250/450/850 UART.
2.  Improve: Prevent the malfunction of serenum driver in Windows 7 x86.
3.  Bugfix: Fixed the bug that diagnostic can't detect CP-104EL, CP-118EL,
    CP-168EL.
4.  Bugfix: Fixed the bug of S/W flow control.
5.  Bugfix: Fixed receive the same data twice when call PurgeComm() after
    ReadFile().

Ver1.18
1. Support CP-104EL-A, CP-168EL-A, CP-118EL-A.

Ver1.17
1. Support CP-114UL-I, CP-112UL, CP-112UL-I

Ver1.16 
1. Official released
2. Support CP-102E, CP-102EL, CP-132EL, CP-132EL-I, CP-114EL, CP-114EL-I

-End-
