
Product:	Smartio,Industio,UPCI and PC/104-Plus Windows NT 4.0 driver
Version:	5.11
Date:		10/07/2007
Company:	Moxa Technologies Co., Ltd


Support Platform:
====================
Windows NT 4.0, i386


Support Product:
====================
CP-102U, CP-102UL
CP-132U-I, CP-132UL,
CP-132, CP-132I, CP132S, CP-132IS, 
CI-132, CI-132I, CI-132IS, 
(C102H, C102HI, C102HIS, C102P, CP-102, CP-102S)

CP-104UL, CP-104JU, CP-114UL, POS-104UL
CP-134U, CP-134U-I
C104H/PCI, C104HS/PCI, 
CP-114, CP-114I, CP-114S, CP-114IS,
C104H, C104HS, 
CI-104J, CI-104JS
CI-134, CI-134I, CI-134IS, 
(C114HI, CT-114I, C104P)

CP-118U, CP-118U-I, CP-138U, CP-138U-I
CP-168U,
C168H/PCI,  
C168H, C168HS, 
(C168P)

CB-108, CB-114, CB-134I


Release Note:
============
Ver5.11
1. Support POS-104UL, CP-138U, CP-138U-I, CP-118U-I, CP-114UL.
2. Support CB-108, CB-114, CB-134I.


Ver5.10
1. Add CP-118U/CP-102UL/CP-102U models. 


Ver5.9 
1. Modify the driver and DLL that can support the FIFO size of MU860 UART. 
2. Driver will set CI-132/CI-134/CI-104J board incorrectly if:
	a. only one board is installed.
	b. JP1 is shorted.
    With the wrong setting, user can't use successive IO address
    with two boards.
    This version fixes this problem. 
    
-End-    

 
    
